KRR Technical Inspection sheet

The engine must be supercharged or turbocharged. Any fuel, any modifications to the engine are allowed. Does engine have a supercharger or a turbocharger? Yes \_\_\_\_ No \_\_\_\_\_

The drive line or shaft must be covered with either 1/8” steel or 1/4” of aluminum. Does the drive shaft covering meet this criteria? Yes \_\_\_\_\_ No \_\_\_\_\_\_

Hull:

Minimum weight shall be 2250 pounds with driver, Actual weight is \_\_\_\_\_\_.

Minimum hull length shall be 17 ft. L.O.A. and the Maximum hull length shall be 20 feet L.O.A. not including cavitation plates. Actual Measurement is \_\_\_\_\_\_\_.

-OR-

When using the optional 21 foot rule, the following rule must be met:

Maximum length 21 feet excluding the cavitation plate. Minimum length 19 feet excluding the cavitation plate. Actual measurement is \_\_\_\_\_\_\_\_\_.

Strake depth must not exceed one and one quarter inch from trailing edge to mid ship. Actual measurement is \_\_\_\_\_\_.

Bottom concavity must not exceed one and one quarter inch from trailing edge to mid ship. Actual measurement is \_\_\_\_\_\_\_.

Nothing must interfere with a straight edge from keel to chine in the area from trailing edge to 65 inches forward. Is this criteria met? Yes \_\_\_\_ No \_\_\_\_\_\_

Dead rise at the transom must not exceed 4 degrees. Actual measurement is \_\_\_\_\_\_\_\_.

All boats meeting this optional 21 foot rule must weigh a minimum of 2,400 pounds. Actual weight is \_\_\_\_\_\_\_\_.

Stabilizers, wing sections or airfoils may be installed, provided they are used in a horizontal position no wider than the beam of the boat under the areas of stabilizer installation. They may not be adjusted while the boat is in motion nor will they be installed to the rear (aft) of the transom. They shall not be positioned forward of amidships. The leading edges shall be no closer than 24 in. from the top of the inside back of the driver’s seat. How close to the driver’s seat is the leading edge? \_\_\_\_\_\_. The leading edge center line shall not be mounted more than 10 in. above the blower(s), injector(s) or top surfaces of other engine top mountings. How close is the leading edge? \_\_\_\_\_\_\_\_.

Chief Inspector APBA #

Inspector APBA #

Referee APBA#

Inboard Commissioner APBA#

Boat Owner’s signature APBA#